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TYPE CERTIFICATE DATA SHEET NO. 29 

This data sheet, which is part of Type Certificate No.29, prescribes conditions and limitations under which the product for which the type certificate was issued meets the airworthiness requirements of the Japan Civil Aeronautics Law and Regulations.

Type Certificate Holder:     Kawasaki Heavy Industries, LTD. (KHI)

3-1-1, Higashi Kawasaki-Cho, Chuo-ku, Kobe-city, Hyogo-prefecture, JAPAN

Model KAWASAKI HUGHES 369D (Normal Category Helicopter, Approved April 20, 1978)

Engine
1(one)  Allison 250-C20B

Fuel
See JCAB Approved Flight Manual for Model KHI 369D.

Engine Ratings & Operating Limits

Takeoff (5 min)
Max. Continuous
Shaft Horsepower:
375SHP
350SHP

Torque:
318ft-lb
297ft-lb


(87.2psi)
(81.3psi)

Gas Producer

  rpm, N1:
53,519rpm (105%)
53,519rpm (105%)

Output Shaft

  rpm, N2:
6,196rpm (103%)
6,196rpm (103%)

Measured Gas Temp.:
1,490°F (810℃)
1,360°F (738℃)


See JCAB approved Flight Manual for other limitations including speed and temperature transients.

Rotor Limits & Engine Operating Speeds
Power Off (Rotor Tach)
Power On (Rotor/Engine Tach)
Maximum: 523 rpm (109% N2)
Maximum: 492 rpm (103% N2)

Minimum: 410 rpm (87% N2)
Minimum: 487 rpm (102% N2)

Airspeed limits (IAS)

VNE (Never Exceed Speed): 288km/h (156kt) IAS

See JCAB approved Flight Manual for reduction of VNE with altitude and temperature.

Center of Gravity (C.G.) Range
Longitudinal
Lateral

Gross Weight
Forward
Aft*
Left
Right

(lb)         
(Sta.)   
(Sta.)
(in.)
(in.)  
3,000
99
103
－3
+3

1,538
99
107.4
－3
+3

Note: Facing forward, + indicates right, and － indicates left of helicopter centerline.

Empty weight C.G. range
None

Maximum weight
3,000 lb.

Minimum crew
1 (Pilot seat: Left hand)

Max. Passengers
5 (1 as pilot, 4 as passengers)
Maximum Cargo
1,300 lb at 115 lb / ft2, Sta. 78.5 to 124

50 lb. evenly distributed in utility storage compartment at Sta. 55.

Fuel capacity
Total Tank Capacity:
416 lb

Usable Fuel Capacity:
403.5lb

Fuel weights are based on JP-4 fuel.

Oil capacity
Engine Oil:
6.00lb (STA133.3in)

Transmission Oil:
11.60lb (STA105.0in)

Maximum Operating Altitude
 16,000 ft (density altitude)

Datum Line
Longitudinal datum (STA.0):
96.89 in forward of forward jacking point.

Horizontal datum (W.L.0):
11.98 in under of forward jacking point.

Rotor Blade and Control Movements
For rigging information refer to the KHI Model 369D Maintenance Instructions.

Serial Numbers Eligible

6701 through 6709 
Certification Basis

KHI has applied for certification on February 14, 1960.

・Civil Aeronautics Regulations Annex 1 “Technical Standards for Ensuring Safety of Aircraft and Equipment.”
・Model KAWASAKI HUGHES 369D of the TAIKUSEI-SINSA-YORYO (JCAB Airworthiness Standards dated
November 14, 1977 (Ku-ken-854).
・Civil Aeronautics Regulations Annex 3 Chapter 1 (equivalent to ICAO Annex 16 Volume 2) for Fuel Venting 
Requirements.
Equipment

Refer to equipment and parts list.
Special Equipment
When equipped with Cargo Hook, or hoist, airworthiness category of "Special Aircraft X" is applied. Refer to the related JCAB approved Flight Manual Supplements.
Publications
JCAB approved Flight Manuals
Maintenance Manual ("Airworthiness limitations" section are JCAB approved.)
Required Equipment
The basic required equipment as prescribed in the applicable Japan Civil Aeronautics Law and Regulations must be installed in the aircraft.
Service Information
Service Bulletins and other service information when JCAB-approved will carry a statement to that effect.
Note: 1   A current Weight & Balance Report must be in each aircraft at the time of original airworthiness 

 certification and at all times thereafter expect in the case of an operator having an JCAB approved 

         loading system for weight and balance control.

Note: 2   Helicopter operation must be in accordance with the JCAB approved Flight Manual. All placards 

 required by either JCAB approved Flight Manual, the applicable operating rules, or the Certification 

         Basis must be installed in the helicopter.
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